v7.2.7

  New digital mode: FHSS Mode

  FHSS Mode is a digital mode based in the FHSS-CDMA modulation.

  It uses 16 different CDMA codes with 1.8 seconds per Hop.

  CAT interface is needed to use this mode.

  Before TX, press the TUNE button and match your antenna in the center of the FHSS band.

  You can select ROS mode or FHSS mode in the frequency menu or in the Frequency Textboxes


  CAT for kenwood TS-570 fixed

  PowerSDR CAT ID should be configured as "TS-2000"

  Alarm tone sounds have been fixed 


  

v7.2.6

  Error13 Bug fixed.   

  AFC set to 200Hz. With the new changes there is no CPU usage difference respect 100Hz

  Tune button relocated over PTT button 

  27635, the only one QRG for 11m
     


v7.2.5

  4 Macro buttons added

  Error10 Bug fixed.

  Internet chat limited. It was damage "the Spirit of Ham radio". 
  In order to do use of your Ham radio License, chat and QSos must be completed 100% via radio, not via internet

  Compass for antenna beams


v7.2.3

  Fixed COM bug with RTS, DTR, and RTS+DTR selection in the Rig menu.

  Less CPU Usage. Now ROS decode 16-8-4 always with less CPU usage.

  Voacap returns. Voacap Coverage Map have been fixed thanks to Jari OH6BG
  Now prediction for ROS consider the effects of the Es layer too.

  3 positions for Waterfall switch:
  Position1: Always ON 
  Position2: Only while decoding (less CPU Usage)
  Position3: Always OFF


v7.2.2

  Beacon answer only with the second CQ call


v7.2.1

  New QRG 27415 for special days


v7.2.0

  CAT control for SmartSDR of Flexradio
 
  Fixed some bugs


v7.1.9

 CAT for Icom IC-7100


v7.1.8

  Spots Configuration Menu

  New Hams included in the Donate screen: F4ABQ, F5LPM, DB4ZW and LU2HAM Many Thanks !



v7.1.7

  Fixed some bugs

  New Hams included in the Donate screen: IW2CX, VK5MHZ, TF2MSN, K4RKM (Opera), 13TH672, IZ0GKZ and G4WCP. Thanks to all
  


v7.1.6

  CAT control for the Yaesu FT3000D

  Changes on 11 meters QRGs:

  27245 USB German QRG
  27610 USB Rest of the world



v7.1.5

  Fixed problems with CAT and user profiles



v7.1.4

  30RC000 11m Cluster conexion. Enable "Cluster" option in ADIF window, or click on skeds to send a Cluster Spot.

  This cluster is activated only if you type a CB callsign


v7.1.3

  27245 (25ch middle) and 27695 (25ch High) for 11 meters band

  Transverter option locked during the transmission



v7.1.2

  Transverter menu for CAT control
 


v7.1.1 

   New QRG for 11 meters: 27245

   New Hams included in the Donate screen: 

  JA1VUC
  HK4GSL
  IK3GIG
  EA4IV  
  JQ1TIV 
  14FRS844 
  DO1OMS
  IZ1LEH 
  OE6KLG
  7L1RLL
  F5OBI 
  29AT133 
  2E0MEG 
  SP3OKS 

  Many thanks to all



v7.1.0 Beta 

  Fixed CAT problem with user change

  Add RST sent and RST recv in ADIF window.

  OE6KLG and 7L1RLL added to Donate list. Thanks to all.



v7.0.9 Beta 

  New QRG for 20m 

  New flags with new names inluded into the Flag folder (Ceuta and Melilla, Korea, and others..)

  IZ1LEH, IK3GIG, EA4IV, JQ1TIV, 14FRS844 AND DO1OMS added to Donate list. Thanks to all.     



v7.0.8 Beta 

  New QRG for 11m 27705


v7.0.7 Beta 

  New DXCC file cty.dat (by Arkady RN6AM). And new Flag folder. 

  DXCC Stats have been updated to the new file.



v7.0.6 Beta 

  No compatible with old versions


v7.0.5 Beta 

  Filter configuration for Kenwood TS-480 fixed (Bug notified by Detlef DL7DET)

  Automatic CQ button 

  HK4GSL added to Donate list. Thanks to the Colombia Connection :-)



v7.0.3 Beta 

  TenTec Pegasus 100% working.

  New QRGs on 80m

  IK8ETN,WB2LMV,EA3GGW,YO5BYV and EA5RQ added to Donate list. Thanks to all.      



v7.0.2 Beta 

  CW ID for the Experimental USA Group and 500Khz licenses.  The macro for CW ID is <CWID>
   


v7.0.1 Beta 

  New DXCC database (by RN6AM). Copy the new "cty.dat" and Flag folder.
  
  Fixed "Error 40016"

  Yaesu FT-100 ready. Thanks to Neil W0YSE by the tests

  Antena selection for IC-775


  SV8QG,G8JNJ,PA0AM,G3RCE,SV1XV,DO1IP,PA0WMR and PA0VRC added to Donate list. Thanks to all.    

  

v7.0.0 Beta 

  Updated to the new ROS server

  New Macro <ALL>. This macro change DECODE switch to "ALL". Recommended to inluce into BYE button, for example


v6.9.7 Beta 

  SWR protection for the next Kenwoods:

  TS-480
  TS-570
  TS-590
  TS-690
  TS-850
  TS-870
  TS-950
  TS-2000

  Now the Arrows in Frecuency dial change bands

  DM2DMI added to Donate list  


v6.9.5 Beta 

  Automatic VFO Compensation system (In Rig menu). Useful for Old Rigs like Kenwood TS-950, TS-440S, etc. 



v6.9.2 Beta 

  PTT via COm for IC-7000, neccesary for Rear Audio input

  PA0OCD, EA6SK and G4ILO included in the Donate List for ROS and Opera Modes. 




v6.9.1 Beta 

   Automatic Compensation SampleRate system. This solve some problems with soundcard when you have open Speclab at the same time
  
   PTT via COM for Kenwood TS-440

   EA3AID and EA6BH included in the Donate List. Gracias Albert nou y Mateo



v6.9.0 Beta 

   Dial Lock Option in Rig menu

   Arranged SWR/PWR display in FT-857 and FT-897. Menu #48 is set to OFF at starting ROS.

   APC system improved

   LU9LB and EA5AIM included in the Donate List. Gracias Jorge y Jesús.



v6.8.8 Beta 

   CAT control for TS-570S and TS-570D.

   Low delay for the S/N meter.

   Arranged the console commands, tested by EA1BAF.



v6.8.6 Beta 

   Arranged problem with Power control in Yaesu FT-450, FT-2000, FT-5000 and FT-9000



v6.8.5 Beta 

   New Macro: <EXPORTQSO>. This is similar to press "EXPORT QSO" button in the ADIF window.

   CAT for Yaesu FT5000D and FT5000MP. If you have any of this rigs please write me to nietoros@hotmail.com  

   In Remote Operation QSO's are saved using the Remote Station (only with the callsign in Remote and Base Station is the same)



v6.8.4 Beta 

   New ROS system improved. Operative from 1 December. No compatible with old versions.

   K3UK and EA5AXZ included in the Donate List. Thanks again.


v6.8.3 Beta 

   Euro Bureau included in QSL via field

   TS-570 at 57600bps

   IZ3SZQ included in the Donate List. Thanks Michel.


v6.8.1 Beta 

   Auto VFOA in Kenwood rigs

   Fixed link to QRZ

   OH3FZQ included in the Donate List. Thanks Michel.


v6.7.9 Beta 

  FT-450D added

  Fixed Width command for FT-2000 and FT-5000

  Fixed frequencies in Logger32


v6.7.8 Beta 

  Fixed a problem with CRC



v6.7.7 Beta 

  Fixed a problem with Profiles in TX: "PORT not available" (reported by EB3JT)

  New QRGs on 40 meters band

  OS3A included in the Donate List. Thanks Michel.


v6.7.4 Beta 

  Fixed a problem in ROS Repeater Operation in the case of change of frequency

  New QRGs for 12m


v6.7.3 Beta 

  QSO forwarding to Cluster

  Improvements in the APC

  HB9MPN and HB9EPE included in the Donate List. Many thanks!



v6.7.1 Beta 

  Fixed a bug of wrong characters in remote operation



v6.7.0 Beta 

  Improvements for the APC



v6.6.9 Beta 

  Fixed "Beacon stopped sometimes".

  Power is written automatically in ADIF windows. Only for CAT users.

  GM3WYL included in the Donate List. Thanks Anthony.



v6.6.8 Beta 

  QSO forwarding for UR5EQF Log, DXKeeper, MIXW2 and Logger32.

  Polish translation by Roman SP4JEU

  New Voacap configuration.

  EA4GDK included in the Donate List. Gracias Agustín  



v6.6.6 Beta 

  Fixed problems in COM detection (Try now with CAT).

  Fixed crap sounds with the ATT 10 dB option

  

v6.6.3 Beta 

  Fixed problems with ROS4 Mode, after the change to the new protocol. 



v6.6.2 Beta 

  Improvements in the Decode Switch (Auto-Timer)

  G3IVB included in the Donate List. Thanks Leslie 



v6.6.1 Beta 

  Improvements in Repeater Mode

  New CTY.dat file and Flag Folder by RN6AM

  OH1KPR included in the Donate List. Many Thanks!     



v6.6.0 Beta 

  New DECODE Switch for selective decoding.

  DECODE to ALL: Decode any message
  DECODE to "EA5HVK": Decode only messages from EA5HVK

  VERY IMPORTANT: This SWITCH will be operative from 3 August. 

  NO COMPATIBLE WITH OLD ROS VERSIONS!!!  Download v6.6.0 as soon as be possible.



v6.5.8 Beta 

  New console for controlling a Remote ROS station via Radio (Console Menu)

  Changes in Repeater Mode. Now users can change the Repeater frequency and band. For example with: R-EA5HVK 7055 Test
  This is only for Repeaters with CAT interface or Softrock TX/RX SDR kit. With no CAT operation, repeater use the same frequency.
  Select Operating Bands in Repeater Menu.

  With the command: "R-EA5HVK BANDS"  you can to know the operating bands in a repeater

  CRC Checksum. All ROS messages are checked using a CRC code. With "<CRC-OK>" message is 100% error free. With "<BAD-CRC>" message has errors

  VERY IMPORTANT: During the first days, the most of messages will appear as "<BAD-CRC>" because old ROS versions have no the CRC.
       
  F5GVA included in the Donate List. Many Thanks!     

  And now, on with the opera



v6.5.7 Beta 

  New Repeater Mode in Repeater Menu. Work as a Parrot in "Iso-Frequency" or "Multi-frequency" (Using CAT or Softrock SDR in this case). 
  Repeater is actived using the RPT switch.
  For using a Repeater Station write at the beguining of your transmission: "R-" + callsign. For example "R-EA5HVK testing repeater Mode"

  New macro <PWR> for the RF Power. CAT interface required.

  Fixed Bugs in Elecraft K3. Tested by Lav LZ1ZJ. Mode must be USB DATA. If you dont know what is DATA mode read the manual.
  
  EA7HGL included in the Donate List. Gracias Antonio.     



v6.5.6 Beta 

  Fixed the green waterfall in Remote Mode

  HB9DPZ included in the Donate List. Many thanks!  



v6.5.5 Beta 
  
  Fine Phase and Gain adjust for SDR kits 

  Waterfall Green Phosphor style (Configuration-->Preferences-->Waterfall)

  CAT for Icom IC-9100 (Tested by EA7HGL)

  USB Mode for Elekcraft K3

  EB1FGO included in the Donate List. Gracias!



v6.5.3 Beta 

  SDR connectivity for SoftRock, KTHSDR, PMSDR, TinySDR, ZetaSDR and the G4JNT LF UpConverter



v6.5.1 Beta 

  New QRG in 6 meters

  Now Underline in the callsigns is according the band.

  Distance and heading at the end of messages

  Beacon Report Mode answer if you call him

  Fixed "VO1" prefix of Canada

  Fixed Antenna Selection on IC-746 (and perhaps also in IC-746 pro)
 
  Fixed filter wideband configuration in Kenwood TS-590

  CT1ARR, KB9YIG, F1RXM and HB0AA have been included in the Donate List. Very grateful to all.
  
  

v6.5.0 Beta 

  Fixed CAT problems for the Icom IC-735 (and 731). Tested by RA3DRC.

  Included CAT for the next old Icom Rigs: IC-78,IC-271,IC-275,IC-375,IC-471,IC-475,IC-575,IC-820,IC-1271,IC-1275

  Included CAT for the Icom IC-RX7 scanner.

  A new donation by LU8EMH, included in the Donate List. Gracias Juan Ramón!



v6.4.9 Beta 

  Fixed a problem in the COM Port list. Notified by HB9MPN and HB9EPE.

  New Private Spot command Line.
   
  EA3WO has been included in the Donate List. Gracias Jesús!. 

  New Donate Window.


v6.4.8 Beta 

   New QRG for 15 meters 21115

   Fixed problem with COM port detected in the EA3WO computer.


v6.4.7 Beta 

   Fixed some bugs


v6.4.6 Beta 

   Diferent CAT configuration for each User Profiles. This is if you have several Rigs connected to ROS.

   Warning Colours for the Vumeter

   PTT via CAT command in the Yaesu FT-920

   GW8ARR, RV3APM and EA3OG have been included in the Donate List. Very grateful.


v6.4.5 Beta 
  
   GPS conection for Portable and Mobile operation (NMEA 0183 Protocol)



v6.4.4 Beta 

   VOACAP Propagation Prediction Map Customized for ROS Mode.

   Translation to Catalá by EA3FHP and EA3OG

   DF1KBN have been included in the Donate List. Many thanks.



v6.4.1 Beta 
  
   Fixed problems with Virtual Ports interfaces. Now ROS CAT can scan until COM Port number 40.

   You have to copy the new OCX folder and run "ROS install v6.4.1.exe". Then ROS can scan your Rig on port 26, for example.

   Information recieved for Yaesu Ft-920 setup was wrong.
   The right setup is: Menu #45 to 0, and Menu #46 to 1170 USB

  

v6.4.0 Beta 

   Distance in miles for some countries



v6.3.8 Beta 

   Improvements in the APC system

   Big Font Size for Transmission Window too

   Automatic /QRP suffix with 5 watts or less (Only for some Rigs)

   HI-SWR speaker sound (Only for some Rigs and windows XP)

   DK8ZV have been included in the Donate List. Many thanks.



v6.3.7 Beta 
  
  APC (Automatic Power Control).

  New file cty.dat and new FLag Folder, with changes in some flags (By RN6AM).

  Waterfall and others functions are disabled temporally when CPU Usage reach 100%. This avoid problems for slow computers 

  CAT for FT-747 and FT-757
  
  PSK Reporter Map v1.4



v6.3.5 Beta 

  Special callsigns accepted in the Database, like TM90RCNF (90th anniversary F8KKH, http://f8kkh.chez-alice.fr/ )



v6.3.4 Beta 

  CAT for TS-590

  Antenna selection by Band. Only for Rigs with two or more antenna connectors.

  On Remote Operation you can RX in all bands, but only TX in the Operating Bands.

  USB Data mode selection for IC-703, IC-746Pro, IC-756Pro2, IC-756Pro3, IC-7200, IC-7400, IC-7600, IC-7700 and IC-7800.

  Detection and Correction of False Spots System. It is in the case of NO CAT operation. 

  Fixed problems closing ROS.

  Fixed "Error 23-5"



v6.3.2 Beta 

  Enabled characters for QTH like (,),#,"ń", etc.... (Operator Menu) 
 
  QSY button in Spot window.

  Fixed some problems with Yaesu FT-897D.

  9600bps for the IC-725 of LU4ECN. Note: This is an inneccesary tunning. CAT works the same to 1200 or 9600bps.



v6.3.0 Beta 

  Direct links to windows audio mixer in soundcard menu

  Fixed error 24. Note, In Remote operation as Base Station if you are not connected with anybody obviously waterfall is paused.

  

v6.2.9 Beta 

  Fixed bugs in Remote Operation


v6.2.8 Beta 

  Frequency restructuring on 40 meters.


v6.2.7 Beta 

  Double Internal Spot System
 
  Disabled DXFUn Cluster.



v6.2.6 Beta 
  
  Frequencies on 30 meters band: 10147, 10148, 10149 (500 Hz)


v6.2.5 Beta 

  ROS Remote operation (see Remote Operation Menu). No aditional audio softwares requeriments.

  Macro for exporting QSO to HAMLOG, HRDLOG, EQSL and ADI file. (see Macro Menu)

  Exporting Selection on ADIF window: .ADI,EQSL, HAMLOG and HRDLOG independently

  Added special frequencies to avoid the the ARRL RTTY "QRP" contest of every weekend (3612, 7110 and 14142)

  Frequency change also if you click on the spot frequency window.

  Fixed CAT for the Yaesu VR-5000 receiver



v6.2.3 Beta 
  
  Audio Input Selection on CAT for IC-703, IC-746Pro, IC-756Pro2, IC-756Pro3 and IC-7800 (Tested by M0ARM)



v6.2.1 Beta 

  Option "Open QSO exported" in HAMLOG.EU (Added by Zoli HA9RQ). 

  Fixed Clear Button (Notified by CO2DC)



v6.2.0 Beta 

  Connectivity with HAMLOG.EU

  ROS.INI is saved in "c:\program files\ROS"
  
  Fixed problems with some Icoms (DG9BFC)  
   

v6.1.9 Beta 

  Fixed the Log files system (Log Menu)

  SWR Protection for the FT1000 MarkV

  Internal Spots enabled for 502 Khz 


v6.1.7 Beta 

  Added CAT for FT-890 

  Fixed Error-22


v6.1.6 Beta 

  Fixed some Bugs in CAT


v6.1.5 Beta 

  Selection of Audio Input (Rear Connector or Mic) in Kenwood Rigs and Yaesu FT847.

  Fixed CAT for TS-570, TS-50, FT847 and some very old Yaesu and Icom interfaces.

  Translation to Romanian. Courtesy of YO4CVV


v6.1.4 Beta 
  
  Connectivity with HRD Loogbook


v6.1.3 Beta 

  Audio output Attenuator of 15 dB (Soundcard menu)


v6.1.2 Beta 

  Fixed problems with some Kenwoods. Automatic configuration of interface parameters.


v6.1.0 Beta 
  
 We have problems with some Kenwood transceivers that we expect to solve in the next days.


v6.0.9 Beta 
  
 RTS High check box for Kenwood and TenTec


v6.0.8 Beta 

  Pyramids was not built in two days. 
  

v6.0.7 Beta 

  Fixed problems in Kenwood.


v6.0.6 Beta 

  Fixed "error 9" changing frequency.

  Preamplifier to OFF below 12 Mhz
  Preamplifier to ON above 12 Mhz


v6.0.4 Beta 

  ROS CAT.

  Frequency for 70cm: 432.097 USB

  

v6.0.3 Beta 

  Found and fixed the next bug: "Microsoft Visual C++ Runtime Libray"


v6.0.2 Beta 

  New AFC Range: ±250Hz & ±100Hz

  I/Q selection warning message. Some ROS users are using of a wrong way Stereo I/Q output with a normal Rig!!
  


v6.0.1 Beta 
  
  New Callsign's Server. Thanks for donations.


v6.0.0 Beta 

  Fixed "Error 380"


v5.9.9 Beta 

  Auto Beacon Spots on DXFunCluster.com/ROS for a better Beacon monitoring. 
  Beacon spot format: Symbol Rate + Timer + Locator + QTH 


v5.9.8 Beta 

  Stereo I/Q output (Soundcard menu). It generates the I/Q output drive for a quadrature upconverter. 


v5.9.7 Beta 

  New frequency for enthusiastic CB users. 27395 Ch.39  


v5.9.6 Beta 
  
  Fixed compatibility with ROS Old Versions ADIF


v5.9.5 Beta 

  DSP Improvements against RTTY interferences. 


v5.9.3 Beta 

  Anti-Jam Switch improves rejection against strong CW and Beacons interferences
  
  It requires more CPU usage and this function is advisable but no essential, so can be disabled if you have and old PC.


v5.9.0 Beta 

  Fixed "Runtime error '340' Control array element '5' doesn't exist"


v5.8.9 Beta 

  Fixed Cuba and Russians countries in DXFunCluster/ROS.


v5.8.8 Beta 

  Fixed problems in ADIF window


v5.8.7 Beta 

  Macro <HISNAME>


v5.8.5 Beta 

  Fixed Runtime Error 5.

  Add 14115

  Ham List in Donate Menu


v5.8.4 Beta 

  New Stats on Stats menu: Number of QSO's, Callsigns and DXCC


v5.7.9 Beta 

  Fixed RunTime error 40006

  Log File modification: An only Log File per day

v5.7.7 Beta 

  New Internal Spot System. You can send Private Messages to others ROS users or Public Messages to all ROS users.

  AutoSpots in this version have been disabled due to pressure of ARRL to remove ROS from the Cluster and, especially, from the waves.
  More info on "http://www.dxcluster.org/"

  ROS Report spots can see monitored internally on the "DXFunCluster website" (Skeds Menu)
  

v5.7.4 Beta

   New Callsigns DataBase Online. Name, QTH and Locator will be filled automatically in ADIF window when you click over a callsign.  
   This system only works for Hams with v5.7.4 or superior.

   New Macro "RPT" to repeat last transmission.
   
   Beacon in Mode Beacon-Report (BRM) only report to CQ Messages


v5.7.1 Beta

   ROS.exe Version for Windows 64 bits.

   Disabled PC Speaker Sounds automatically in the case of Windows 7.

   Fixed a problem with "QSL_COMMENT" ADIF field and HRD.


v5.7.0 Beta
 
  Fixed problems with Windows7 and Realtek soundcard. 
   

v5.6.9 Beta

  By suggestion of John G4BAV, when scanning continues after decoding a signal, it would be nice if the frequency of the decoded signal was displayed against it so that you would know where to look for the station again.

  By suggestion of Julio Cesar CT1BWI, a sound is played when the RX message is for you.

  Now in Alarm/sound Menu you can configure multiples sounds. So, you can monitoring ROS activity all day with the software minimized in your PC.
  For example, a sound is played when a DXCC not worked appear in the RX text.

  Changes on 40 meters.

  Paypal Donate Link on Help Menu. Donations are Welcome.


v5.6.8 Beta

  "Clear TX" option for Macro Buttons. This is for, when you press the button, TX window was erased.

   ROS is now compatible with "Win98" and "Milenium", except the "CPU usage" meter. For this reason, Beacon only can works in "Report Only Mode" (ROM)


v5.6.7 Beta

   You can Rename or Delete some Macro Buttons. To delete a Macro button, delete the name.


v5.6.6 Beta

  "Name", "QTH" and "Locator" are automatically detected and inserted in ADIF window for the 95% of cases.
   In the 5% of cases you will have to fill the fields by the conventional way (see Help/Shortcuts Menu)

   Re-translation to Russian by Arkady RN6AM.

  

v5.6.3 Beta

  New Macros (Run "ROS Install.exe") 


v5.6.2 Beta

  By suggestion of Joseph Levy, .INI file remember the sound-cards of the different USERs

  Changes in Menus. It requires run "install.exe" to register "Hook-Menu-2.ocx"
  
  New frequency for 80 meters: 3583.

v5.6.1 Beta

   Now "ROS.INI" is saved in c:\Documents and Settings\All Users\ROS\ROS.ini
   In the case of Windows 7, it is saved in "C:\ProgramData\Ros\Ros.ini" 


v5.5.7 Beta

  Now QSO's are not duplicated when you import the ADIF file to HRD selecting "ignore duplicates".
  If you have old ROS QSO's stored in HRD, you can save it to an ADIF file and copy a paste into ROS.adi file.
  In the case of MIXw or FlDigi you have no any problem with duplicates too. 

  So, do no delete ROS.adi after import QSO's to preserve the information.

  Re-translation to French by F4BSX
  
  By suggestion of Adriaan PE2KP, ADIF Button on Main Panel

  By suggestion of Fabien ON6CF, User Profiles for 8 users

  By suggestion of F6HBW, SCAN automaticaly start again after a reception 

  ROS Facebook link on Help Menu

  Definitivelly, ROS doesn't work in Windows 98 and Windows Milenium. There is no way of registering "PDH.DLL".
  If you know how do it, all yours.



v5.5.6 Beta

  Fixed Log File system

v5.5.4 Beta

  Fixed the country in portable callsigns like "E7/DJ1US/M", etc..

v5.5.0 Beta

  By suggestion of Craig KQ6I, User Profiles (I think 4 users is enough)

  Translation to Hungarian by Biro Tamas HG1DFB. Many thanks. 
  

v5.4.9 Beta

  Doing click, now also get callsigns like "/QRP" /M" etc..  

  New frequencies for 40 an 80 meters.

  Roger Beep sounds when you recieve a Cluster Spot. Only when Alarm Switch is ON.

  Waterfall is automatically disabled when CPU Usage is too high in your PC. A message will appear in the screen.
  
  Included "pdh.dll" in "install.exe" for Windows Millenium


v5.4.7 Beta
 
  Fixed some problems with the soundcard control

  Different Colours for RX window

  New frequency for 20 meters: 14101

  Included "psapi.dll" in "install.exe" for Windows Millenium
  
  Note: File "cluster.exe" is no longer necessary in the new versions.

v5.4.4 Beta
   
  A new Display appears when somebody send you a Cluster Spot for you.
  Press in "Note icon" to hide/show the message
  Press in the "PC Monitor icon" to reply quickly is you wish.

  Link to QRZ/callsign

  CAT adapted to "Yaesu FT-100 D". If you have questions, ssk in ROS CAT support: digicat@egopa.com

v5.4.2 Beta

  Fixed 14113 and 18113 buttons.

v5.4.1 Beta

   By suggestion of Luis EA5DOM, Omnirig works with two CATS syncronized at the same frecuency.
   He uses a SDR to receive and a FT-897 to transmit, both controlled by CAT.
  

v5.4.0 Beta

  Soundcard sliders. Improvements in Soundcard selection. 

  For people that don't look at the CPU Meter, in Beacon Mode Waterfall is disabled automatically when CPU usage is too high.

  A lot of new flags by Arkady, RN6AM. Replace your old Flag Folder by the new Flag folder.


v5.3.9 Beta

  Fixed a bug in the Omnirig file for the Yaesu FT-817 (By Emilio, EB4FMT). If you have a FT-817, run "install.exe".

  Fixed a bug in CountDown Beacon visibility.


v5.3.8 Beta


  Tone switch in Main panel
  

v5.3.5 Beta

  Improvements in Countries Database. Thanks to Arkady,RN6AM
  New flags has been included

v5.3.4 Beta

  Add Countries and Flags.

  Number of Countries worked with ROS, in Stats menu.

  Callsigns of countries didn't work, appear in red color. 

  7055 is replaced by 7046 

v5.3.2 Beta

  New frequency for 4 meters: 70.074 Mhz

  14091 is replaced by 14079

  Fixed a bug in windows frequencies direct links 

  Beacon improvements:
  RX Symbol-Rate is always switched to 16-8-4 when you use the beacon. It avoid interfering with users that work in 4 bauds.
  Beacon is disabled if your PC is too slow to decode. 
  Some people are using old PC's exclusively for transmitting a beacon without any possibility of decode right, so they can interfere to others users.
  New changes avoid this situation.   


v5.3.1 Beta
  
  New frequency: 10145. Use it when 10144 was busy (don't interfere with others ROS users, please).

  ROS CAT support in Rig Menu (by EB4FMT). Ask your questions in "digicat@egopa.com" if you have problems with CAT configuration 

v5.3.0 Beta
  
  Now you can send the QSO to "eQSL.cc"at the same time you export the QSO to ADIF. 
  It requires run "install.exe" if you have problems with some DLL.


v5.2.1 Beta
  
  Fixed a bug on the 3598 frecuency

v5.2.0 Beta

  "Cancel Frame Button" appears during the reception. Press this button if you wish cut the message (Or "Esc" key)

  Improvements in CAT. Now you can switch the frequency using "Page Up" or "Page down" without delay.

v5.1.1 Beta

  Option CAT via VOX

v5.1.0 Beta

  New file "Cluster.exe" to avoid problems of saturation on 18 and 15 meters. Sorry for the inconvenience and "Mea culpa".

  Three new frequencies: 7048(500Hz), 18114(2000Hz) and 21114(2000Hz) 

  Now, shortcuts to change the frequency are: "Page Up" and "Page Down"


v5.0.0 Beta

  Compatible with Windows2000 (except PSK Reporter function)

  To avoid saturation, new frequency on 20 meters: 14091 (500Hz). Remember going to other frequency when the channel was busy by others users.

  New Shortcuts: With "Page Up" and "Page Down" you can change the frequency (if you use CAT)

  Changes in "Log Menu". Select in "Log Menu" if you wish Save a Log File or not. "Save Log Button" is not necessary.


v4.9.9 Beta

  Some people was using the beacon without RX possibility, so beacon could interfere.
  The new Beacon System doesn't let to the beacon transmit if you dont have a right Input Volume Level. In that case, the CountDown will never goes to zero.

  Changes in the protocol. ROS 2250Hz now is ROS 2000Hz (since August, 13) 

  Note: Cancel Frame Button have dissapeared to avoid people interfere between them in a feedback cycle.
  If somebody is doing a QSO in a channel, please QSY to other channel o wait for your turn.


v4.9.8 Beta

  Baud has been inserted in CLuster Spots. It requires replace the file "Cluster.exe"

v4.9.7 Beta

  Fixed a bug changing of frequency. Thanks again to Jorge EA8TL.  

v4.9.6 Beta
   
  Direct link to DX Fun Cluster/ROS in Skeds Menu. Thanks to JAVI EC4DX and Jorge EA8TL.

  By suggestion of Ińaki EA2CVV, Frequency inserted in Log file.

  ROSMF audio and test tone now centered in 1500Hz.

v4.9.5 Beta
   
  New frequency for 20 Meters: 14078 (BW:500Hz according with IARU Band Plans)

v4.9.4 Beta

  Fixed bug in CAT when you opened ROS. For example: Runtime Error 5 and friends. 
  Thanks to Emilio EB5DBW for lending the Yaesu FT857 to fix the CAT.

  Fixed a bug "in RX window have not been underlined callsigns with which already QSO". Thanks to Arkady RN6AM again. 

v4.9.2 Beta

  Fixed "ROS QSO's Stats" in Stat menu. Thanks to RN6AM for the report.


v4.9.1 Beta

  Fixed a bug that deleted the text in the beacon when 2 beacons were running in the same channel.
  Also, a Standard Beacon message is added automatically for people that don't know how use the beacon.

  ADIF path modified. It Requires you open "LOG/ADIF menu" again to select the file .adi

  Some changes in macros.
 

v4.9.0 Beta

  Control "MCI32.OCX" has been included in the installation.
  Run "install.exe" if you had problems with this OCX. 

v4.8.9 Beta
  
  New Alarm Menu. If you have 2 soundcard you can select a sound file as alarm instead of Pc Speaker.
  
  Beacon menu simplyfied with Beacon timer until 10 minutes.

  Default Button in Macros Menu to load Macros by default.


v4.8.8 Beta

  Fixed a bug in the Callsign Detection. 

  Translation to Euskera (Ahí va la ostia :-) ). Courtesy of Humberto Arteche EA2HA


v4.8.7 Beta

  Fixed a bug in PSKReporter. Many spots were not being sent to the map. New file "PSKReporter.exe"

v4.8.5 Beta

  If you don't have CAT also can write frequency manually in the Frequency Box  

v4.8.4 Beta
  
  If you don't have CAT you must select the frequency manually using "Frequencies Menu" or in the direct link for 20 meters.


v4.8.3 Beta

   Cluster window on "Skeds Menu".
         

v4.8.2 Beta

   ROS has been joined to PSK Automatic Propagation Reporter. It requires run install.exe
   You have a direct link in "Skeds menu".

   Thanks to Philip Gladstone N1DQ for his help and patience.


v4.7.5 Beta
  
  Fixed spot frequency with CAT.

v4.7.4 Beta

  Fixed a bug in ADIF frequency

v4.7.0 Beta

  By suggestion of CO2DC and "The man of the Vara" I will continue to develop ROS. 

  A new Sked page have been linked to ROS software.  


